Bestxyz processor

User Manual

Edwards AFB, CIV USAF 412 RANS/ENRTE (USA)

Written By: Hannselthill Camacho (Student Trainee)

[1. SETUP INFORMATION 1](#_Toc46837392)

[1.1 Physical Equipment 1](#_Toc46837393)

[1.2 Compatible Operating Systems 1](#_Toc46837394)

[1.3 User Provided Information 1](#_Toc46837395)

# SETUP INFORMATION

## 1.1 Physical Equipment

A modern computer or laptop capable of running windows 10 operating system is required to run the application.

## 1.2 Compatible Operating Systems

The application has been tested and created to work in a windows 10 environment. The application has not been tested in Linux, Mac, or earlier versions of windows OS.

## 1.3 User Provided Information

The user is expected to have a reference receiver dataset that follows the [OEM7 Commands and Logs Reference Manual](https://docs.novatel.com/oem7/Content/Home.htm) message specifications.

The user is expected to provide the Earth Centered Earth Fixed E, F, and G coordinates by either loading them from a valid file or manually inputting them into the provided text fields in the GUI.

## 1.4 Installation Steps

Extract the “BestXYZ\_Processor\_V1.0\_Release.zip” file into the desired location on your local computer. Go to the newly extracted file directory and then into the “release” directory. Inside you will find the “Project\_1.exe”. Run the executable to start the application.